Section: Lowcut Filters

The Lowcut Filters are usually situated on a Crossover Device, but Pro Graph 32 has it's own Filters. Checking this option sets a negative value of -5db on all Frequencies lower than 25Hz. Any adjustment you have made to the Bandwidth Control may prevent the Filter from working as intended. No restrictions are in place to prevent this. You have complete control of what you are creating.